FDDI(CDDI)¥High speed network interface: 100 Mb/s¥Uses 4B/5B coding—Maps each 4 bits of data into a 5 bit pattern for transmission,e.g. 1111 --> 11101—Line rate is 125 M symbols/s¥Priority operation is the simular to the token bus scheme

FDDI(CDDI)¥Multiple token operation

PDU

PDU

Token

PDU

PDU

PDU

Token