¥IEEE 802.3 [10 Mb/s]—CSMA/CD—Baseband

—Token Bus—Modulated¥IEEE 802.5 [4 and 16 Mb/s]—Token ring

¥IEEE 802.6 [typically 45 Mb/s]—Dual Queue Dual Bus (DQDB)¥FDDI (CDDI) [100 Mb/s]

—Copper Distributed Data Interface—Baseband¥LATM [variable]¥IEEE 802.12 [100 Mb/s]

Network LayerIEEE 802.2Medium Access ControlPhysical LayerIEEE 802.2 = Logical Link Control