1Collision Free Protocols¥Collision free protocolsestablish rules to determinewhich stations sends after asuccessful transmission.

with unique addresses 0 to N-1.

¥A contention intervalis a periodafter a successful transmissionthat is divided into N time slots,one for each station.

2Collision Free Protocols¥If a station has a PDU to send itsets a bit to 1 in its time slot inthe contention interval.¥

data to send and the order in

which it will be sent.

Contention

Interval 26 811111

3Collision Free Protocols¥Problems:—Fairness—